# Version 1.0 Changelog –

1. AHU HCAI –
   1. Added
   2. Added a custom supply return exhaust air logic that considers the exhaust from the room, desired air balance and other stuff to automate supply CFM return CFM and exhaust CFM.
   3. OA cfm and additional CFM on the top (used to change the OSA % of the AHU) are now linked automatically when you add an AHU.
   4. Freeze protection logic fixed.
2. AHU Multizone –
   1. Updated pop up to select options.
   2. Freeze protection logic fixed.
   3. Unchecking reheat coil in the AHU removes it from the schedule.
   4. Checking the AHU reheat coil still looks at the mixed air temperature and indicates if it is not needed.
   5. Added desired air balance from the room (+ve -ve amount)
   6. Fixed diversity of the people with one Ps value, instead of Ps on all zones.
   7. Added a misc. exhaust column.
   8. Fixed how EX is calculated. Adds misc exhaust now.
   9. Fixed how DCV CFM is calculated. Now it considers if there is no CO2 sensor in the room.
   10. Fixed Co2 sensor. Note the CO2 sensor requirement is from 2022 ASHRAE.
   11. Added a custom supply return exhaust air logic that considers the exhaust from the room, desired air balance and other stuff to automate supply CFM return CFM and exhaust CFM.